{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["设备成本明细","安装成本明细"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"设备成本明细","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8],[5,0,9,0],[5,1,7,1],[10,0,15,0],[10,1,12,1],[16,0,20,0],[21,0,31,0],[35,0,35,8],[36,0,36,8],[37,0,37,8]],"flags":["formulas_cached_only"]}
["《项目现场物料统计表》"]
["项目名称：雅安人民医院第三院(一进一出2.0)"]
["项目地址："]
["项目负责人联系电话："]
["类型","序号","设备名称","规格型号","安装数量","单价","总价","供货方","备注"]
["入口设备",1,"直杆道闸","TTX-DZ-ZG001",1,null,0,"停天下","方向：    正向    长度：4米"]
[null,null,"广告道闸","TTX-DZ-GG001",null,null,0,null,"方向：         长度："]
[null,null,"栅栏道闸","TTX-DZ-ZL001",null,null,0,null,"方向：         长度："]
[null,2,"识别一体机R型","TTX-R",1,null,0," ","4.0版本显示和语音，补光灯"]
[null,3,"高清车牌识别相机","TTX-RM",1,null,0," ","臻识"]
["出口设备",1,"直杆道闸","TTX-DZ-ZG001",1,null,0,"停天下","方向：         长度：4米"]
[null,null,"广告道闸","TTX-DZ-GG001",null,null,0,null,"方向：         长度："]
[null,null,"栅栏道闸","TTX-DZ-ZL001",null,null,0,null,"方向：         长度："]
[null,2,"识别一体机R型","TTX-R",1,null,0," ","4.0版本显示和语音，补光灯"]
[null,3,"高清车牌识别相机","TTX-TCG225",1,null,0," ","臻识"]
[null,4,"收费机","TTX-SFJ-001",null,null,0]
["集中控制设备",1,"停天下工控机","TTX-PC-16",1,null,0,null,"Linux一台"]
[null,2,"硬盘刻录机","TTX-camera8",0,null,0,null,"海康威视8路网络硬盘录像机"]
[null,3,"路由器","TTX-LANSW",1,null,0,null,"1000M路由器"]
[null,4,"交换机","TTX-JHJ",2,null,0]
[null,5,"人行翼闸","TTX-RXDZ001",null,null,0,null,"翼闸+摆闸"]
["辅助材料",1,"停天下隔离柱","TTX-GLZ",null,null,0,null,"（配新纪元膨胀螺丝1根隔离柱3个）"]
[null,2,"停天下锥形桶","TTX-ZXT",null,null,0,null," "]
[null,3,"辅助相机","TTX-RM",0,null,0,null," "]
[null,4,"辅助相机立柱","TTX-LZ-RM",0,null,0,null," "]
[null,5,"安防相机","TTX-AFXJ",0,null,0,null," "]
[null,6,"安防相机立柱","TTX-AFXJ-LZ",0,null,0,null," "]
[null,7,"出入口指示牌","TTX-ZSP-01",null,null,0,null," "]
[null,8,"场内支付二维码","TTX-IN-QRCODE",10,null,0,null," "]
[null,9,"语音提示器","TTX-TSQ-SOUND",null,null,0,null," "]
[null,10,"车检器","TTX-CJQ",2,null,0,null," "]
[null,11,"空气开关","TTX-KQKG",2,null,0,null," "]
[null,12,"雷达车检器","TTX-LDCJQ",null,null,0]
[null,null,"运费",{"$nulls":3},0,null," "]
["总价",{"$nulls":5},0,null," "]
[]
["                                                                   工程技术人员签字：陈勇"]
["                                                                     "]

{"sheet":"安装成本明细","index":1,"n_rows":32,"n_cols":8,"rows_kept":32,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,1],[2,2,2,4],[2,5,2,6],[3,2,3,4],[32,0,32,7]],"flags":["formulas_cached_only"]}
["外包安装工程成本核算表"]
["所有安装需要的辅材，包括但不限于：电源线、网线、地感线、膨胀钉、水泥辅材等，都由工程承包方提供。以下价格包含辅料价格。"]
["项目名称：雅安人民医院第三院(一进一出2.0)",null,"施工单位：",null,null,"负责人：",null,"时间：2020年7月13日"]
["工程部经理（签字）：",null,"商务总监（签字）：",null,null,"财务（签字）：",null,"总经理（签字）："]
["序号","名目","工程类型","单 位","数量","综合单价","合 价(元）","备注"]
[1,"雅安人民医院第三院","1进1出"]
[2,"道闸机安装",null,"个",2,0,0]
[3,"识别一体机安装",null,"个",2]
[4,"辅助相机",null,"个",0]
[5,"安防相机",null,"个",0]
[6,"指示牌",null,"个",0]
[7,"出口收费机",null,"台",0]
[8,"混泥土开槽",null,"米",5]
[9,"电源线BRV2*1平方护套线",null,"米",40]
[10,"混凝土或沥青地感线圈开槽深度5CM（5圈）2M*1M",null,"个",4]
[11,"地砖或石材地感线圈开槽深度10CM（5圈）2M*1M",null,"个",0]
[12,"网线（包括穿管）",null,"米",50]
[13,"挖土、填土",null,"米",0]
[14,"设备岛建设费",null,"平方",1]
[15,"设备岛刷漆",null,"平方",0]
[16,"车道刷标志线（含漆、稀释剂、辅料工具）",null,"单道",0]
[17,"隔离柱",null,"根",0]
[18,"四芯光缆（包括穿管）",null,"米",0]
[19,"电源线BRV2*2.5平方护套线（包括穿管）",null,"米",0]
[20,"光纤熔纤费",null,"次",0]
[21,"光纤终端盒",null,"个",0]
[22,"光纤尾纤",null,"根",0]
[23,"雷达车检器",null,"个",0]
[24,"原设备拆除",null,"次",0]
[25,"外地指导安装及调试",null,"天",0,0,0]
[null,"合计",{"$nulls":4},0]
[null,"实际合计",{"$nulls":4},0]